2019 MDI Photo Club Exhibit (continued}


2025 MDI Photo Club Exhibit 

Ready to be Hung Requirements

Ideal:
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Attach wire anchor 1/4 to 1/3 down 
from the top of the frame.



The wire when pulled taut 
towards the top of the frame 
should be no closer than two inches from the top of the frame. 
This will hide the hanging hardware when hung in the Mellon Room.




Figure 1 Perfect
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Figure 2 Also Good Metal Print with Float Mount



[image: High%20Wire.jpg]Figure 3 Wire too slack







Wire is too close to top of frame when pulled taught.
















[image: ]Figure 4 High Wire







Wire attachments are too close to top of frame and wire has insufficient slack.








[image: Canvas.jpg]

D-ring clips mounted on back face are also acceptable.
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Figure 5 Canvas Print Methods
Sawtooth hangers are not acceptable.
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Figure 6 Sawtooth – NO

Questions about “ready to hang” should be directed to Caitlin Small at (401) 225-7407 or exhibit@mdiphotoclub.org. 
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